

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Horsepower: | Length: | Beam: | Deep Draft: | Astern Bollard: | Ahead Bollard: |
| 1,320 | **60’** | **23’** | **9’** | **13.12 Kips** | **19.58 Kips** |
| Engines: | **Face Wires:** | **Fresh Water:** | **Fuel Oil:** |
| Twin CumminsQSK19-M | **7/8”x110’** |  |  |
| Propellers: | **Anchor Wire:** | **Anchor Winch:** |
| Twin | **7/8”x50’** | **50,000 lbs. (Bow)** |
| Gross Tonnage: | **Call Sign:** | **Official Number:** |
| 63 | **WBC6570** | **285752** |
| Note: |
|  |