

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Horsepower: | Length: | Beam: | Deep Draft: | Astern Bollard: | Ahead Bollard: |
| 1,320 | **60’** | **23’** | **9’** | **13.12 Kips** | **19.58 Kips** |
| Engines: | **Face Wires:** | | | **Fresh Water:** | **Fuel Oil:** |
| Twin Cummins  QSK19-M | **7/8”x110’** | | |  |  |
| Propellers: | **Anchor Wire:** | | | **Anchor Winch:** | |
| Twin | **7/8”x50’** | | | **50,000 lbs. (Bow)** | |
| Gross Tonnage: | **Call Sign:** | | | **Official Number:** | |
| 63 | **WBC6570** | | | **285752** | |
| Note: | | | | | |
|  | | | | | |