

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Horsepower: | Length: | Beam: | Deep Draft: | Astern Bollard: | Ahead Bollard: |
| 880 | **72’** | **21’** | **3.5** |  |  |
| Engines: | **Face Wires:** | **Fresh Water:** | **Fuel Oil:** |
| Twin CumminsN14M | **7/8”x110’** |  |  |
| Propellers: | **Tow Winch:** | **Anchor Winch:** |
| Twin Nozzles |  | **50,000 lbs. (Bow)** |
| Gross Tonnage: | **Call Sign:** | **Official Number:** |
| 56 | **WCY8255** | **1067220** |
| Note: |
|  |