

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Horsepower: | Length: | Beam: | Deep Draft: | Astern Bollard: | Ahead Bollard: |
| 880 | **72’** | **21’** | **3.5** |  |  |
| Engines: | **Face Wires:** | | | **Fresh Water:** | **Fuel Oil:** |
| Twin Cummins  N14M | **7/8”x110’** | | |  |  |
| Propellers: | **Tow Winch:** | | | **Anchor Winch:** | |
| Twin Nozzles |  | | | **50,000 lbs. (Bow)** | |
| Gross Tonnage: | **Call Sign:** | | | **Official Number:** | |
| 56 | **WCY8255** | | | **1067220** | |
| Note: | | | | | |
|  | | | | | |