

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Horsepower: | Length: | Beam: | Deep Draft: | Astern Bollard: | Ahead Bollard: |
| 3,000 | **100’** | **33’** | **12’** | **43.86 Kips** | **65.53 Kips** |
| Engines: | **Rudders:** | | | **Fresh Water:** | **Fuel Oil:** |
| Twin EMD  12-645-E6 | **Twin** | | |  |  |
| Propellers: | **Plasma Pennants:** | | | **Face Wires:** | |
| Twin | **Forward 40’**  **Aft 52’** | | | **1”x75’** | |
| Gross Tonnage: | **Call Sign:** | | | **Official Number:** | |
| 145 | **WCC9851** | | | **583761** | |
| Note: | | | | | |
| Tank Vessel Escort Certified | | | | | |