

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Horsepower: | Length: | Beam: | Deep Draft: | Astern Bollard: | Ahead Bollard: |
| 3,000 | **79’** | **25’** | **11’** | **39.50 Kips** | **61.11 Kips** |
| Engines: | **Face Wires:** | | | **Fresh Water:** | **Fuel Oil:** |
| Twin Cummins  KTA38-M2 | **1”x110’** | | |  |  |
| Propellers: | **Main Tow Wire:** | | | **Under-Rider Wire:** | |
| Twin | **1.5”x1300’** | | | **1.5”x600’** | |
| Gross Tonnage: | **Call Sign:** | | | **Official Number:** | |
| 92 | **WBR6265** | | | **600562** | |
| Note: | | | | | |
| Tank Vessel Escort Certified | | | | | |