

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Horsepower: | Length: | Beam: | Deep Draft: | Astern Bollard: | Ahead Bollard: |
| 3,000 | **79’** | **25’** | **11’** | **39.50 Kips** | **61.11 Kips** |
| Engines: | **Face Wires:** | **Fresh Water:** | **Fuel Oil:** |
| Twin CumminsKTA38-M2 | **1”x110’** |  |  |
| Propellers: | **Main Tow Wire:** | **Under-Rider Wire:** |
| Twin | **1.5”x1300’** | **1.5”x600’** |
| Gross Tonnage: | **Call Sign:** | **Official Number:** |
| 92 | **WBR6265** | **600562** |
| Note: |
| Tank Vessel Escort Certified |