

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Horsepower: | Length: | Beam: | Deep Draft: | Astern Bollard: | Ahead Bollard: |
| 3,900 | **124’** | **31’5”** | **15’** | **74.94 Kips** | **105 Kips** |
| Engines: | **Rudders:** | | | **Fresh Water:** | **Fuel Oil:** |
| Twin EMD 16-645-E2 | **Quad** | | | **8,000 Gal.** | **75,000 Gal.** |
| Propellers: | **Tow Winch:** | | | **Bow Winch:** | |
| 96”x112” Nozzles | **Single Drum 2,600 of 2-1/4 Wire**  **110,000 Lbs. at 60 FPM** | | | **1-Drum**  **2-Gypsies** | |
| Gross Tonnage: | **Call Sign:** | | | **Official Number:** | |
| 180 | **WDD8770** | | | **506606** | |
| Note: | | | | | |
| Tank Vessel Escort Certified | | | | | |