

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Horsepower: | Length: | Beam: | Deep Draft: | Astern Bollard: | Ahead Bollard: |
| 2,000 | **65’** | **24’** | **8’** |  |  |
| Engines: | **Face Wires:** | **Fresh Water:** | **Fuel Oil:** |
| Twin CumminsKTA38-M1 | **7/8”x110’** |  |  |
| Propellers: | **Anchor Wire:** | **Anchor Winch:** |
| Twin Nozzles | **7/8”x50’** | **50,000 lbs. (Bow)** |
| Gross Tonnage: | **Call Sign:** | **Official Number:** |
| 150 | **WCY5602** | **569110** |
| Note: |
|  |