

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Horsepower: | Length: | Beam: | Deep Draft: | Astern Bollard: | Ahead Bollard: |
| 1,320 | **75’** | **24’** | **8’** | **25.0 Kips** | **35.0 Kips** |
| Engines: | **Rudders:** |  | **Fresh Water:** | **Fuel Oil:** |
| Twin CumminsQSK19-M | **Twin** | **3,000 Gal.** | **21,000 Gal.** |
| Propellers: | **Main Tow Wire:** | **Under-Rider Wire:** |
| Twin Kort Nozzles | **1.5”x2500’** | **1.5”x600’** |
| Gross Tonnage: | **Call Sign:** | **Official Number:** |
| 116 | **WDB6361** | **599924** |
| Note: |
| Tank Vessel Escort Certified |