

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Horsepower: | Length: | Beam: | Deep Draft: | Astern Bollard: | Ahead Bollard: |
| 1,320 | **75’** | **24’** | **8’** | **25.0 Kips** | **35.0 Kips** |
| Engines: | **Rudders:** |  | | **Fresh Water:** | **Fuel Oil:** |
| Twin Cummins  QSK19-M | **Twin** | | | **3,000 Gal.** | **21,000 Gal.** |
| Propellers: | **Main Tow Wire:** | | | **Under-Rider Wire:** | |
| Twin  Kort Nozzles | **1.5”x2500’** | | | **1.5”x600’** | |
| Gross Tonnage: | **Call Sign:** | | | **Official Number:** | |
| 116 | **WDB6361** | | | **599924** | |
| Note: | | | | | |
| Tank Vessel Escort Certified | | | | | |