

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Horsepower: | Length: | Beam: | Deep Draft: | Astern Bollard: | Ahead Bollard: |
| 1,550 | **70’5”** | **26’** | **8’5”** | **21.16 Kips** |  |
| Engines: | **Face Wires:** | | | **Fresh Water:** | **Fuel Oil:** |
| Twin Cat.  3508E | **1”x110’** | | |  |  |
| Propellers: | **Anchor Wire:** | | | **Anchor Winch:** | |
| Twin | **7/8”x50’** | | | **50,000 lbs. (Bow)** | |
| Gross Tonnage: | **Call Sign:** | | | **Official Number:** | |
| 148 | **WDB5141** | | | **530049** | |
| Note: | | | | | |
|  | | | | | |