

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Horsepower: | Length: | Beam: | Deep Draft: | Astern Bollard: | Ahead Bollard: |
| 880/Single Push Knee | **56’** | **15’** | **5’** | **15.17 Kips** | **19.77 Kips** |
| Engines: | **Face Wires:** | **Fresh Water:** | **Fuel Oil:** |
| Twin CumminsN14M | **7/8x75’** |  |  |
| Propellers: | **Tow Winch:** | **Bow Winch:** |
| Twin Nozzles |  |  |
| Gross Tonnage: | **Call Sign:** | **Official Number:** |
| 30 | **WCY5209** | **269531** |
| Note: |
|  |