

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Horsepower: | Length: | Beam: | Deep Draft: | Astern Bollard: | Ahead Bollard: |
| 880/Single Push Knee | **56’** | **15’** | **5’** | **15.17 Kips** | **19.77 Kips** |
| Engines: | **Face Wires:** | | | **Fresh Water:** | **Fuel Oil:** |
| Twin Cummins  N14M | **7/8x75’** | | |  |  |
| Propellers: | **Tow Winch:** | | | **Bow Winch:** | |
| Twin Nozzles |  | | |  | |
| Gross Tonnage: | **Call Sign:** | | | **Official Number:** | |
| 30 | **WCY5209** | | | **269531** | |
| Note: | | | | | |
|  | | | | | |