

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Horsepower: | Length: | Beam: | Deep Draft: | Astern Bollard: | Ahead Bollard: |
| 1,050 | **65’** | **19’** | **5’** |  |  |
| Engines: | **Face Wires:** | | | **Fresh Water:** | **Fuel Oil:** |
| Twin Cummins  KTA-1150 | **7/8”x110’** | | |  |  |
| Propellers: | **Anchor Wire:** | | | **Anchor Winch:** | |
| Twin | **7/8”x75’** | | |  | |
| Gross Tonnage: | **Call Sign:** | | | **Official Number:** | |
| 63 | **WZX5454** | | | **521657** | |
| Note: | | | | | |
|  | | | | | |