

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Horsepower: | Length: | Beam: | Deep Draft: | Astern Bollard: | Ahead Bollard: |
| 1,550 | **70’5”** | **26’** | **8’5”** | **21.16 Kips** |  |
| Engines: | **Face Wires:** | **Fresh Water:** | **Fuel Oil:** |
| Twin Cat.3508E | **1”x110’** |  |  |
| Propellers: | **Anchor Wire:** | **Anchor Winch:** |
| Twin | **7/8”x50’** | **50,000 lbs. (Bow)** |
| Gross Tonnage: | **Call Sign:** | **Official Number:** |
| 148 | **WDB5141** | **530049** |
| Note: |
|  |